Installation et configuration d'un rpi0w avec une connexion vpn :

$ date && sudo dd bs=1M if=2017-03-02-raspbian-jessie-lite.img of=/dev/sdb && date
dimanche 2 avril 2017, 21:11:05 (UTC+0200)
1329+0 enregistrements lus
1329+0 enregistrements écrits
1393557504 bytes (1,4 GB, 1,3 GiB) copied, 156,685 s, 8,9 MB/s
dimanche 2 avril 2017, 21:13:42 (UTC+0200)

Configuration post installation : Attention de la clavier est en qwerty donc pour le mot de passe il faut mettre q au lieu de a et pour le - il faut taper sur ° au lieu de 6

sudo raspi-config

Configuration du wifi en ligne de commande :

Configurer simplement le wifi d’un Raspberry PI sous Raspbian en CLI

$ sudo nano /etc/wpa_supplicant/wpa_supplicant.conf

country=FR
ctrl_interface=DIR=/var/run/wpa_supplicant GROUP=netdev
update_config=1
network={
ssid="MONWIFI"
psk="MONPASSEWIFI"
id_str="nomdemonwifi"
}

$ sudo nano /etc/network/interfaces

# interfaces(5) file used by ifup(8) and ifdown(8)
# Please note that this file is written to be used with dhcpcd
# For static IP, consult /etc/dhcpcd.conf and 'man dhcpcd.conf'
# Include files from /etc/network/interfaces.d:
source-directory /etc/network/interfaces.d
auto lo
iface lo inet loopback
iface eth0 inet manual
allow-hotplug wlan0
iface wlan0 inet manual
wpa-conf /etc/wpa_supplicant/wpa_supplicant.conf
allow-hotplug wlan1
iface wlan1 inet manual
wpa-conf /etc/wpa_supplicant/wpa_supplicant.conf
# Wifi nomdemonwifi
iface nomdemonwifi inet dhcp

$ sudo reboot

$ ifconfig wlan0

sudo apt update && sudo apt upgrade -y && sudo apt dist-upgrade -y && sudo apt install rpi-update && sudo apt-get clean && sudo apt-get autoremove && sudo df -h

sudo rpi-update

sudo apt-get install openvpn && sudo mkdir /etc/openvpn/monvpn

sudo apt install htop screen rpi-update -y